**Seat Pivot Black Plastic Slide fitted under Bolster Seats.**

**(Note: Recall does not apply to non-Bolster Seat installations)**

**Date of sale:** Sold by Bar Crusher Boats and Bar Crusher Boat’s dealers fitted to bolster style seats between March 2014 and November 2016.

**Defect:** The black plastic pivot / slide mechanism fitted under the bolster style seat that acts as the mounting mechanism to the seat box tube, may crack under very heavy loads and extreme forces.

**Hazard:** If the pivot / slide mechanism cracks and fails, the seat could detach from the seat box and pose a fall hazard to consumers.

**What to do:** Inspect the black plastic mechanism for cracks and if any are identified do not use the seat until the pivot is replaced. If you have this style of pivot / slide mechanism fitted under your BOLSTER seats, consumers should contact Bar Crusher boats via the web address below to register for rectification.

**Contact Details: C**ontact Bar Crusher Boats by emailing your contact details with “Safety Recall” as the subject to [info@barcrusher.com.au](file:///C%3A%5CUsers%5Cthorn%5CAppData%5CLocal%5CMicrosoft%5CWindows%5CTemporary%20Internet%20Files%5CContent.Outlook%5CZTJ00EL9%5Cinfo%40barcrusher.com.au) and Bar Crusher will provide advice and guidance to remedy the matter.

**Your email will need to provide the following information:**

1. Your name, mailing address and phone contact.
2. Model of boat.
3. HIN Number from HIN plate at rear of engine pod.

In addition, you may call Bar Crusher on **03 9792 2999** for advice 11.00am to 4.00pm Monday to Friday however, registration for recall is still requested online.